; MiiSW4.INF  -- Windows Still Image Setup File for ScanMaker 8700/X12USL Scanners
; Note - this file is for Windows 98/98SE/ME/2000/XP only.
; Copyright (c) 2002 Microtek International, Inc.

[Version]
LayoutFile=layout.inf, layout1.inf, layout2.inf
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Mfg%
DriverVer=02/04/2002,1.00.0001.1
CatalogFile=MiiSW4.cat

[ControlFlags]
ExcludeFromSelect=*

[SourceDisksNames]
168=%DiskName%,,

[SourceDisksFiles]
MSMB0W.dll=168
MSMB1w.dll=168
MSMWUD.DLL=168
miiscan.sys=168
MSMUSD5.dll=168
scsi1394.sys=168

[DestinationDirs]
; By default, files will be copied to \windows\system.
DefaultDestDir=11
;For 98
STI98MSMUSD5.CopyFiles=11
SCSI_98.CopySys32Files=10,system32\drivers
USB_98.CopySys32Files=10,system32\drivers
scsi1394_98.CopySys32Files=10,system32\drivers  ; LDID_WIN\SYSTEM32\DRIVERS
;For 2000
STI_MSMUSD5.CopyFiles=11
USB_2000.CopySys32Files=10,system32\drivers
;For WIA
USB.WIA.CopySys32Files=10,system32\drivers

[Manufacturer]
%Mfg%=Models, NT.5.1

[Models]
;For 98
%USB\VID_05DA&PID_20B0.DeviceDesc%=X12USL_USB,USB\VID_05DA&PID_20B0
%SCSI\________SCANMAKER_X12USL1.DeviceDesc%=X12USL_SCSI,________SCANMAKER_X12USL1
%SCSI\________SCANMAKER_X12USL0.DeviceDesc%=X12USL_SCSI,________SCANMAKER_X12USL0
%SBP2\0000D0B9&00B1.DeviceDesc%=SM8700_1394,SBP2\0000D0B9&00B1&CmdSetId104d8
%USB\VID_05DA&PID_20B1.DeviceDesc%=SM8700_USB,USB\VID_05DA&PID_20B1

;For WIA
%USB\VID_05DA&PID_20B0.DeviceDesc%=X12USL_USB.WIA,USB\VID_05DA&PID_20B0
%SCSI\________SCANMAKER_X12USL1.DeviceDesc%=X12USL_SCSI.WIA,________SCANMAKER_X12USL1
%SCSI\________SCANMAKER_X12USL0.DeviceDesc%=X12USL_SCSI.WIA,________SCANMAKER_X12USL0
%SBP2\0000D0B9&00B1.DeviceDesc%=SM8700_1394.WIA,SBP2\0000D0B9&00B1&CmdSetId104d8
%USB\VID_05DA&PID_20B1.DeviceDesc%=SM8700_USB.WIA,USB\VID_05DA&PID_20B1

;For Windows XP(Whistler) or later. (NTWIA)
[Models.NT.5.1]
%USB\VID_05DA&PID_20B0.DeviceDesc%=X12USL_USB.NTWIA,USB\VID_05DA&PID_20B0
%SCSI\________SCANMAKER_X12USL1.DeviceDesc%=X12USL_SCSI.NTWIA,________SCANMAKER_X12USL1
%SCSI\________SCANMAKER_X12USL0.DeviceDesc%=X12USL_SCSI.NTWIA,________SCANMAKER_X12USL0
%SBP2\0000D0B9&00B1.DeviceDesc%=SM8700_1394.NTWIA,SBP2\0000D0B9&00B1&CmdSetId104d8
%USB\VID_05DA&PID_20B1.DeviceDesc%=SM8700_USB.NTWIA,USB\VID_05DA&PID_20B1

[STI.Scanner.AddWinIni]
win.ini,Microtek,,"Interface=STI",0

;*************************************************************************************
;            For Win98, 98SE
;*************************************************************************************
[X12USL_SCSI]
DriverVer=02/01/2002,1.00.0001.1
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=Microtek.Events.GOButton
DeviceData=X12USL_SCSI.DeviceData
AddReg=SCSI_98.AddReg
CopyFiles=X12USL_98.CopyFiles,STI98MSMUSD5.CopyFiles,SCSI_98.CopySys32Files
DeviceSubType=0x0101
;ICMProfiles="sRGB Color Space Profile.icm"
DelFiles=X12USL_98.CopyFiles
UpdateInis=STI.Scanner.AddWinIni

[X12USL_SCSI.Services]
AddService = scsiscan, 0x00000002, scsiscan.AddService

[X12USL_SCSI.DeviceData]
TwainDS=%ScanWizard32%
Type=0

[scsiscan.AddService]
DisplayName    = %scsiscan.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\scsiscan.sys
LoadOrderGroup = Base

[SCSI_98.AddReg]
;HKR,,HardwareConfig,1,2
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,"scsimap.sys,scsiscan.sys"
;
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek SCSI Scanner"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMUSD5.dll
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,"Apartment"
;----------------------------------------------------------------
[SM8700_USB]
DriverVer=02/01/2002,1.00.0001.1
SubClass=StillImage
DeviceType=1
Capabilities=3
DeviceData=SM8700_USB.DeviceData
AddReg=USB_98MSMUSD5.AddReg
CopyFiles=SM8700_98.CopyFiles,STI98MSMUSD5.CopyFiles,USB_98.CopySys32Files
DelFiles=SM8700_98.CopyFiles
DeviceSubType=0x0101
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[SM8700_USB.DeviceData]
TwainDS=%ScanWizard32%
Type=0
PortType=5

[SM8700_USB.Services]
AddService = miiscan, 0x00000002, usbscan.AddService

[X12USL_USB]
DriverVer=02/01/2002,1.00.0001.1
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=Microtek.Events.GOButton
DeviceData=X12USL_USB.DeviceData
AddReg=USB_98MSMUSD5.AddReg
CopyFiles=X12USL_98.CopyFiles,STI98MSMUSD5.CopyFiles,USB_98.CopySys32Files
DelFiles=X12USL_98.CopyFiles
DeviceSubType=0x0101
;ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[X12USL_USB.DeviceData]
TwainDS=%ScanWizard32%
Model=MCS-1200XU
Type=0

[X12USL_USB.Services]
AddService = miiscan, 0x00000002, usbscan.AddService

[usbscan.AddService]
DisplayName    = %usbscan.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\miiscan.sys
LoadOrderGroup = Base

[USB_98MSMUSD5.AddReg]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,MIISCAN.SYS
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek USB Scanner"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMUSD5.dll
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,"Apartment"
;----------------------------------------------------------------------------
[SM8700_1394]
DriverVer=02/01/2002,1.00.0001.1
SubClass=StillImage
DeviceType=1
Capabilities=3
DeviceData=SM8700_1394.DeviceData
AddReg=1394_98.AddReg
CopyFiles=SM8700_98.CopyFiles,STI98MSMUSD5.CopyFiles,scsi1394_98.CopySys32Files
DelFiles=SM8700_98.CopyFiles
DeviceSubType=0x0101
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[SM8700_1394.Services]
AddService = scsi1394, 0x00000002, scsi1394.AddService

[SM8700_1394.DeviceData]
TwainDS=%ScanWizard32%
Type=0
PortType=9

[scsi1394.AddService]
DisplayName    = %scsi1394.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\scsi1394.sys
LoadOrderGroup = Base

[RestoreSTI]
CopyFiles=STIUSD.CopyFiles

[1394_98.AddReg]
;HKR,,HardwareConfig,1,2
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,scsi1394.sys
;
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek FireWire Scanner"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMUSD5.dll
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,"Apartment"
;----------------------------------------------------------------------------
[X12USL_98.CopyFiles]
;MSMB0W.dll

[SM8700_98.CopyFiles]
;MSMB1w.dll

[STI98MSMUSD5.CopyFiles]
MSMUSD5.dll

[USB_98.CopySys32Files]
miiscan.sys

[scsi1394_98.CopySys32Files]
scsi1394.sys

[SCSI_98.CopySys32Files]
scsimap.sys
scsiscan.sys

;*************************************************************************************
;            For Win2000
;*************************************************************************************
[X12USL_SCSI.NT]
DriverVer=02/04/2002,1.00.0001.1
Include=    sti.inf
Needs= STI.SCSISection
SubClass=StillImage
DeviceType=1
Capabilities=3
DeviceData=X12USL_SCSI.NT.DeviceData
AddReg=SCSI_2000.AddReg
Events=Microtek.Events.GOButton
CopyFiles=X12USL_2000.CopyFiles,STI_MSMUSD5.CopyFiles,SCSI.Sys32.CopyFiles
DelFiles=X12USL_2000.CopyFiles
DeviceSubType=0x0101
;ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[X12USL_SCSI.NT.Services]
Include=    sti.inf
Needs= STI.SCSISection.Services

[X12USL_SCSI.NT.DeviceData]
TwainDS=%ScanWizard32%
Type=0

[SCSI_2000.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,"SCSISCAN.SYS"
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek SCSI Scanner"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMUSD5.dll
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,"Apartment"
;----------------------------------------------------------------------------
[SM8700_USB.NT]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x0101
Capabilities=3
DeviceData=SM8700_USB.NT.DeviceData
AddReg=USB_2000MSMUSD5.AddReg
CopyFiles=SM8700_2000.CopyFiles,STI_MSMUSD5.CopyFiles,USB_2000.CopySys32Files
DelFiles=SM8700_2000.CopyFiles
UpdateInis=STI.Scanner.AddWinIni
;ICMProfiles="sRGB Color Space Profile.icm"

[SM8700_USB.NT.DeviceData]
TwainDS=%ScanWizard32%
Type=0
PortType=5

[SM8700_USB.NT.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[X12USL_USB.NT]
DriverVer=02/04/2002,1.00.0001.1
Include=    sti.inf
Needs= STI.USBSection
SubClass=StillImage
DeviceType=1
Capabilities=3
DeviceData=X12USL_USB.NT.DeviceData
AddReg=USB_2000MSMUSD5.AddReg
CopyFiles=X12USL_2000.CopyFiles,STI_MSMUSD5.CopyFiles,USB_2000.CopySys32Files
DelFiles=X12USL_2000.CopyFiles
;ICMProfiles="sRGB Color Space Profile.icm"
Events=Microtek.Events.GOButton
UpdateInis=STI.Scanner.AddWinIni

[X12USL_USB.NT.Services]
Include=    sti.inf
Needs= STI.USBSection.Services

[X12USL_USB.NT.DeviceData]
TwainDS=%ScanWizard32%
Type=0

[USB_2000MSMUSD5.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,"USBSCAN.SYS"
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek USB Scanner"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMUSD5.dll
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,"Apartment"
;----------------------------------------------------------------------------
[SM8700_1394.NT]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.SCSISection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x0101
Capabilities=3
DeviceData=SM8700_1394.NT.DeviceData
AddReg=1394_2000.AddReg
CopyFiles=SM8700_2000.CopyFiles,STI_MSMUSD5.CopyFiles
DelFiles=SM8700_2000.CopyFiles
UpdateInis=STI.Scanner.AddWinIni
;ICMProfiles="sRGB Color Space Profile.icm"

[SM8700_1394.NT.DeviceData]
TwainDS=%ScanWizard32%
Type=0
PortType=9

[SM8700_1394.NT.Services]
Include=sti.inf
Needs=STI.SCSISection.Services

[1394_2000.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,"SCSISCAN.SYS"
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek FireWire Scanner"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMUSD5.dll
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,"Apartment"

[X12USL_2000.CopyFiles]

[SM8700_2000.CopyFiles]

[SCSI.Sys32.CopyFiles]

[STI_MSMUSD5.CopyFiles]
MSMUSD5.dll

[USB_2000.CopySys32Files]
;usbscan.sys

;*************************************************************************************
;            For WIA
;*************************************************************************************
[X12USL_SCSI.WIA]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.SCSISection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x13
Events=Microtek.Events.GOButton
DeviceData=X12USL_SCSI.WIA.DeviceData
AddReg=SCSI_WIA.AddReg
CopyFiles=X12USL_WIA.CopyFiles,USD.WIA.CopyFiles
DelFiles=X12USL_WIA.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[X12USL_SCSI.WIA.Services]
Include=sti.inf
Needs=STI.SCSISection.Services

[X12USL_SCSI.WIA.DeviceData]
Server=local
UI DLL=sti.dll
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}
PortType=3

[SCSI_WIA.AddReg]
;HKR,,DevLoader,,*NTKERN
;HKR,,NTMPDriver,,"SCSISCAN.SYS"
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek STI USD Driver"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMWUD.DLL
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,Both
;---------------------------------------------------
[SM8700_USB.WIA]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x10
DeviceData=SM8700_USB.WIA.DeviceData
AddReg=USB_WIA.AddReg
CopyFiles=SM8700_WIA.CopyFiles,USD.WIA.CopyFiles,USB.WIA.CopySys32Files
DelFiles=SM8700_WIA.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[SM8700_USB.WIA.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[SM8700_USB.WIA.DeviceData]
Server=local
UI DLL=sti.dll
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}
PortType=5

[X12USL_USB.WIA]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x13
Events=Microtek.Events.GOButton
DeviceData=X12USL_USB.WIA.DeviceData
AddReg=USB_WIA.AddReg
CopyFiles=X12USL_WIA.CopyFiles,USD.WIA.CopyFiles,USB.WIA.CopySys32Files
DelFiles=X12USL_WIA.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[X12USL_USB.WIA.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[X12USL_USB.WIA.DeviceData]
Server=local
UI DLL=sti.dll
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}
PortType=5

[USB_WIA.AddReg]
;HKR,,DevLoader,,*NTKERN
;HKR,,NTMPDriver,,"USBSCAN.SYS"
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek STI USD Driver"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMWUD.DLL
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,Both
;---------------------------------------------------
[SM8700_1394.WIA]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.SBP2Section
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x10
DeviceData=SM8700_1394.WIA.DeviceData
AddReg=SBP2_WIA.AddReg
CopyFiles=SM8700_WIA.CopyFiles,USD.WIA.CopyFiles,SBP2.CopySys32Files
DelFiles=SM8700_WIA.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[SM8700_1394.WIA.Services]
Include=sti.inf
Needs=STI.SBP2Section.Services

[SM8700_1394.WIA.DeviceData]
Server=local
UI DLL=sti.dll
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}
PortType=9

[SBP2_WIA.AddReg]
;HKR,,DevLoader,,*NTKERN
;HKR,,NTMPDriver,,"SCSI1394.SYS"
HKR,,USDClass,,"{66CFF0C0-A94B-11d1-808C-0000E816F968}"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968},,,"Microtek STI USD Driver"
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,,,%11%\MSMWUD.DLL
HKCR,CLSID\{66CFF0C0-A94B-11d1-808C-0000E816F968}\InProcServer32,ThreadingModel,,Both

;*************************************************************************************
;            For Windows XP NTWIA
;*************************************************************************************
[X12USL_SCSI.NTWIA]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.SCSISection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x13
Events=Microtek.Events.GOButton
DeviceData=X12USL_SCSI.WIA.DeviceData
AddReg=SCSI_WIA.AddReg
CopyFiles=X12USL_WIA.CopyFiles,USD.WIA.CopyFiles
;DelFiles=X12USL_WIA.CopyFiles
UninstallSection=Uninstall.X12USL_XP
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[X12USL_SCSI.NTWIA.Services]
Include=sti.inf
Needs=STI.SCSISection.Services

[Uninstall.X12USL_XP]
DelFiles=X12USL_WIA.CopyFiles
;---------------------------------------------------
[SM8700_USB.NTWIA]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x10
DeviceData=SM8700_USB.WIA.DeviceData
AddReg=USB_WIA.AddReg
CopyFiles=SM8700_WIA.CopyFiles,USD.WIA.CopyFiles,USB.WIA.CopySys32Files
;DelFiles=SM8700_WIA.CopyFiles
UninstallSection=Uninstall.SM8700_XP
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[SM8700_USB.NTWIA.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[Uninstall.SM8700_XP]
DelFiles=SM8700_WIA.CopyFiles

[X12USL_USB.NTWIA]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x13
Events=Microtek.Events.GOButton
DeviceData=X12USL_USB.WIA.DeviceData
AddReg=USB_WIA.AddReg
CopyFiles=X12USL_WIA.CopyFiles,USD.WIA.CopyFiles,USB.WIA.CopySys32Files
;DelFiles=X12USL_WIA.CopyFiles
UninstallSection=Uninstall.X12USL_XP
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[X12USL_USB.NTWIA.Services]
Include=sti.inf
Needs=STI.USBSection.Services
;---------------------------------------------------
[SM8700_1394.NTWIA]
DriverVer=02/04/2002,1.00.0001.1
Include=sti.inf
Needs=STI.SBP2Section
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x10
DeviceData=SM8700_1394.WIA.DeviceData
AddReg=SBP2_WIA.AddReg
CopyFiles=SM8700_WIA.CopyFiles,USD.WIA.CopyFiles,SBP2.CopySys32Files
;DelFiles=SM8700_WIA.CopyFiles
UninstallSection=Uninstall.SM8700_XP
ICMProfiles="sRGB Color Space Profile.icm"
UpdateInis=STI.Scanner.AddWinIni

[SM8700_1394.NTWIA.Services]
Include=sti.inf
Needs=STI.SBP2Section.Services
;---------------------------------------------------
[X12USL_WIA.CopyFiles]
MSMB0w.dll

[SM8700_WIA.CopyFiles]
MSMB1w.dll

[USD.WIA.CopyFiles]
MSMWUD.DLL

[USB.WIA.CopySys32Files]
;USBSCAN.SYS

[SBP2.CopySys32Files]
;SBP2SCAN.SYS
;---------------------------------------------------
[Microtek.Events.GOButton]
Event0=%Button%,{099183A0-AEB5-11d1-B964-0000E816F968},*

[Strings]
Msft="Microsoft"
Mfg="Microtek"

Button="Go Button"

scsiscan.SvcDesc = "SCSI Scanner Driver"
usbscan.SvcDesc = "USB Scanner Driver"
scsi1394.SvcDesc = "FireWire Scanner Driver"
ScanWizard32="Microtek ScanWizard Pro"
DiskName = "Microtek Scanning Software"

SBP2\0000D0B9&00B1.DeviceDesc = "Microtek ScanMaker 8700 (FireWire)"
USB\VID_05DA&PID_20B1.DeviceDesc = "Microtek ScanMaker 8700 (USB)"
USB\VID_05DA&PID_20B0.DeviceDesc="Microtek ScanMaker X12USL"
USB\VID_05DA&PID_20EE.DeviceDesc="Microtek ScanMaker X12USL"
SCSI\________SCANMAKER_X12USL1.DeviceDesc = "Microtek ScanMaker X12USL"
SCSI\________SCANMAKER_X12USL0.DeviceDesc = "Microtek ScanMaker X12USL"