; Windows Modem Setup File
; Copyright (c) 1993-1996 Microsoft Corporation
; Manufacturer: Sierra Semiconductor

[Version]
LayoutFile=layout.inf
Signature="$CHICAGO$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Sierra%

[Manufacturer]
%Sierra% = Sierra

[ControlFlags]
ExcludeFromSelect=UNIMODEM6A25C644   ; Sierra, AST
ExcludeFromSelect=ISAPNP\SSC0001_DEV0000
ExcludeFromSelect=ISAPNP\SSC0000_DEV0000
ExcludeFromSelect=ISAPNP\SSC0004_DEV0000
ExcludeFromSelect=UNIMODEM3B65849A   ; Sierra

[Modem2.PosDup]
*PNP0500

[Modem288.PosDup]
*PNP0500

[Sierra]
%Modem1% = Modem1, UNIMODEM527EBE7A               ; SQ3223
%Modem2% = Modem2, SIER_Modem2, UNIMODEM6A25C644  ; SQ3229
%Modem3% = Modem2, ISAPNP\SSC0001_DEV0000         ; SQ3262
%Modem3% = Modem2, SIER_Modem3, UNIMODEM6A25C644  ; SQ3262
%Modem4% = Modem2, SIER_Modem4, ISAPNP\SSC0000_DEV0000         ; SQ3228
%Modem4% = Modem2, SIER_Modem4, UNIMODEM6A25C644  ; SQ3228
%Modem5% = Modem2, UNIMODEM6A25C644               ; Sierra, AST
%Modem6% = Modem2, ISAPNP\SSC0004_DEV0000         ; SQ3230
%Modem6% = Modem2, SIER_Modem6, UNIMODEM6A25C644  ; SQ3230
%SQ3465% = Modem288, ISAPNP\SSC0101_DEV0000
%SQ3465% = Modem288, UNIMODEM3B65849A

[Modem1]        
AddReg=All, MfgAddReg, Modem1.AddReg, INTERNAL

[Modem2]
AddReg=All, MfgAddReg, Modem2.AddReg, INTERNAL

[Modem288]
AddReg=All, MfgAddReg, Mod288AddReg, VoiceAll, VoiceV34, INTERNAL
CopyFiles= DLL_FILES

[Modem1.AddReg]         
HKR,, Properties, 1, 80,01,00,00, 3c,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, 40,38,00,00
HKR, Settings, Compression_On,, "%%C3"

[Modem2.AddReg]
HKR,, Properties, 1, 80,01,00,00, 3c,00,00,00, 5a,00,00,00, 07,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, 40,38,00,00
HKR, Settings, ErrorControl_On,, "\N6"

[Mod288AddReg]
HKR,, Properties, 1, 80,01,00,00, FF,00,00,00, 00,00,00,00, 07,00,00,00, 0F,00,00,00, 37,03,00,00, 00,C2,01,00, 80,70,00,00
HKR,, DCB, 1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00,0A,00, 0a,00,08,00, 00,11,13,00, 00,00,32,2D
HKR, Init, 2,, "AT &F S0=0 E0 &C1 &D2 \V0 \T0 &H0<cr>"
HKR, Settings, ErrorControl_Forced,, "\N5\V2"   
HKR, Settings, FlowControl_Off,,"\Q0" 
HKR, Settings, FlowControl_Hard,,"\Q3"
HKR, Settings, FlowControl_Soft,,"\Q1"

[VoiceAll]
HKR,,Enumerator,,serwave.vxd
HKR,,TrainingDLL,,spktrn16.dll
HKR,, VoiceProfile,          1, 27,20,91,01
HKR,, VoiceBaudRate,         1, 00,c2,01,00
HKR, VoiceHangup, 1,, "at#vh=0<cr>"
HKR, VoiceHangup, 2,, "at#vs0<cr>"
HKR, VoiceHangup, 3,, "ATZ<cr>"
HKR,, SpeakerPhoneSpecs,       1, ff,00,00,00,  00,00,00,00,  80,00,00,00,  00,00,00,00
HKR, SpeakerPhoneEnable,      1,, "atm2<cr>"
HKR, SpeakerPhoneEnable,      2,, "at#vm=1<cr>"
HKR, SpeakerPhoneDisable,     1,, "atm0<cr>"
HKR, SpeakerPhoneDisable,     2,, "at#vm=0<cr>"
HKR, SpeakerPhoneDisable,     3,, "at#spm=0<cr>"
HKR, SpeakerPhoneMute,        1,, "at#vm=0<cr>"
HKR, SpeakerPhoneUnMute,      1,, "at#vm=1<cr>"
HKR, SpeakerPhoneSetVolumeGain,  1,, "at#spv=<Vol><cr>"
HKR, SpeakerPhoneSetVolumeGain,  2,, "at#spg=<Gain><cr>"
HKR, StartPlay,               1,, "at#vsv<cr>"
HKR, StopPlay,                1,, "None"
HKR, StopPlay,                2,, "NoResponse"
HKR, StartRecord,             1,, "at#vd1<cr>"
HKR, StopRecord,              1,, "None"
HKR, StopRecord,              2,, "NoResponse"
HKR,, TerminateRecord,,      "<h10><h03>"
HKR,, TerminatePlay,,        "<h10><h03>"
HKR,, AbortPlay,,            "<h10><h18><h10><h03>"
HKR,, HandsetCloseDelay,	1, 03,00,00,00
HKR, OpenHandset,             1,, "at#vs1<cr>"
HKR, OpenHandset,             2,, "at#vh=2<cr>"
HKR, OpenHandset,             3,, "atm0<cr>"
HKR, LineSetPlayFormat,       1,, "at#vsm=2<cr>"
HKR, LineSetPlayFormat,       2,, "at#vsc=0<cr>"
HKR, LineSetPlayFormat,       3,, "at#vss=2<cr>"
HKR, LineSetPlayFormat,       4,, "at#vbo=1<cr>"
HKR, LineSetPlayFormat,       5,, "at#vti=0<cr>"
HKR, HandsetSetPlayFormat,    1,, "at#vsm=2<cr>"
HKR, HandsetSetPlayFormat,    2,, "at#vsc=0<cr>"
HKR, HandsetSetPlayFormat,    3,, "at#vss=2<cr>"
HKR, HandsetSetPlayFormat,    4,, "at#vbo=1<cr>"
HKR, HandsetSetPlayFormat,    5,, "at#vh=2<cr>"

HKR,, ForwardDelay,            1,88,13
HKR, CloseHandset,              1,, "at#vh=0<cr>"
HKR, CloseHandset,              2,, "at#vs0<cr>"
HKR, CloseHandset,              3,, "atM2<cr>"
HKR, VoiceToDataAnswer,         1,, "at#vs0<cr>"
HKR, VoiceToDataAnswer,         2,, "ata<cr>"

HKR, VoiceAnswer,               1,, "at#vs1<cr>"
HKR, VoiceAnswer,               2,, "atm0<cr>"
HKR, VoiceAnswer,               3,, "at#vaa=4<cr>"
HKR, VoiceAnswer,	        4,, "at#vat=1<cr>"
HKR, VoiceAnswer,               5,, "at#vt1<cr>"
HKR, VoiceAnswer,               6,, "ata<cr>"
HKR, VoiceAnswer,               7,, "at#vbo=1<cr>"
HKR, VoiceAnswer,               8,, "at#vti=0<cr>"

HKR, WaveDriver,  BaudRate       ,1, 00, c2, 01, 00
HKR, WaveDriver,  XformID        ,1, 08, 00, 00, 00
HKR, WaveDriver,  XformModule    ,, "umdmxfrm.dll"
HKR, WaveDriver,  WaveHardwareID ,, "SierraVoiceModemWave"
HKR, Sierra,  DefaultTimeout      ,1, d0, 07, 00, 00
HKR, Sierra,  DefaultResponse      ,, <cr><lf>OK<cr><lf>
HKR, Sierra\Reset,  Command      ,, atz<cr>
HKR, Sierra\EchoOff,  Command      ,, ate0<cr>
HKR, Sierra\VoiceEnable,  Command      ,, at#vs1<cr>
HKR, Sierra\SpeakerPhoneEnable,  Command      ,, "at#spm=1<cr>"
HKR, Sierra\DownLoad,  Command      ,, "at#spu=2<cr>"
HKR, Sierra\UpLoad,  Command      ,, "at#spd=2<cr>"
HKR, Sierra\UpLoad,  Response     ,, ""
HKR, Sierra\Train,  Command      ,, "at#spt=2,t91<cr>"
HKR, Sierra\Train,  Response     ,, "<cr><lf>OK<cr><lf>"
HKR, Sierra\Train,  Timeout     ,1, 30, 75, 00, 00
HKR, Sierra\SetTrainData,  Command      ,, "at#spu=5<cr>"
HKR, Sierra\TrainingQuery,  Command      ,, "at#spt?<cr>"
HKR, Sierra\Answer,         Command      ,, "ata<cr>"
HKR, Sierra\Answer,         Response     ,, "<cr><lf>#VCON<cr><lf>"
HKR, VoiceDialNumberSetup, 1,, "at#vs1<cr>"
HKR, VoiceDialNumberSetup, 2,, "at#vt1<cr>"
HKR, VoiceDialNumberSetup, 3,, "at#vrn=0<cr>"
HKR, VoiceDialNumberSetup, 4,, "at#vbo=1<cr>"
HKR, VoiceDialNumberSetup, 5,, "at#vti=0#vtr=255<cr>"
HKR, VoiceDialNumberSetup, 6,, "ats6=1<cr>"
HKR, AutoVoiceDialNumberSetup, 1,, "at#vs1<cr>"
HKR, AutoVoiceDialNumberSetup, 2,, "at#vt1<cr>"
HKR, AutoVoiceDialNumberSetup, 3,, "at#vrn=60<cr>"
HKR, AutoVoiceDialNumberSetup, 4,, "at#vra=50<cr>"
HKR, AutoVoiceDialNumberSetup, 5,, "at#vbo=1<cr>"
HKR, EnableDistinctiveRing, 1,, "at#vs1<cr>"
HKR, EnableDistinctiveRing, 2,, "at#vdr=1,10<cr>"
HKR, EnableDistinctiveRing, 3,, "at#vs0<cr>"
HKR, GenerateDigit,               1,, "atx3dt<Digit>;<cr>"
HKR, EnableCallerID,               1,, "at#cc1<cr>"
HKR,, CallerIDPrivate,,P
HKR,, CallerIDOutSide,,O
HKR,, VariableTerminator,,<cr><lf>
HKR, Responses, "<cr><lf>#VCON<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "DATE= ", 1, 93, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "TIME= ", 1, 94, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "CID= ", 1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NAME= ", 1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "MESG= ", 1, 97, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "DRON=", 1, 91, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "DROF=", 1, 92, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>#VD0<cr><lf>",        1, 1b, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>#VD1<cr><lf>",        1, 1b, 00, 00,00,00,00, 01,00,00,00
HKR, Responses, "<cr><lf>#VD2<cr><lf>",        1, 1b, 00, 00,00,00,00, 02,00,00,00
HKR, Responses, "<cr><lf>#VD3<cr><lf>",        1, 1b, 00, 00,00,00,00, 03,00,00,00
HKR, Responses, "<cr><lf>#VD4<cr><lf>",        1, 1b, 00, 00,00,00,00, 04,00,00,00
HKR, Responses, "<cr><lf>#VD5<cr><lf>",        1, 1b, 00, 00,00,00,00, 05,00,00,00
HKR, Responses, "<cr><lf>#VD6<cr><lf>",        1, 1b, 00, 00,00,00,00, 06,00,00,00
HKR, Responses, "<cr><lf>#VD7<cr><lf>",        1, 1b, 00, 00,00,00,00, 07,00,00,00
HKR, Responses, "<cr><lf>#VD8<cr><lf>",        1, 1b, 00, 00,00,00,00, 08,00,00,00
HKR, Responses, "<cr><lf>#VD9<cr><lf>",        1, 1b, 00, 00,00,00,00, 09,00,00,00
HKR, Responses, "<cr><lf>#VD*<cr><lf>",        1, 1b, 00, 00,00,00,00, 0e,00,00,00
HKR, Responses, "<cr><lf>#VD#<cr><lf>",        1, 1b, 00, 00,00,00,00, 0f,00,00,00
HKR, Responses, "<cr><lf>#VDA<cr><lf>",        1, 1b, 00, 00,00,00,00, 0a,00,00,00
HKR, Responses, "<cr><lf>#VDB<cr><lf>",        1, 1b, 00, 00,00,00,00, 0b,00,00,00
HKR, Responses, "<cr><lf>#VDC<cr><lf>",        1, 1b, 00, 00,00,00,00, 0c,00,00,00
HKR, Responses, "<cr><lf>#VDD<cr><lf>",        1, 1b, 00, 00,00,00,00, 0d,00,00,00
HKR, Responses, "<cr><lf>#VIR<cr><lf>",        1, 1b, 00, 00,00,00,00, 2d,00,00,00
HKR, Responses, "<cr><lf>#VDG<cr><lf>",        1, 1b, 00, 00,00,00,00, 27,00,00,00
HKR, Responses, "<cr><lf>#VIL<cr><lf>",        1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>#VIS<cr><lf>",        1, 1b, 00, 00,00,00,00, 2d,00,00,00
HKR, Responses, "<cr><lf>#VTH<cr><lf>",        1, 1b, 00, 00,00,00,00, 22,00,00,00
HKR, Responses, "<cr><lf>#VTO<cr><lf>",        1, 1b, 00, 00,00,00,00, 21,00,00,00
HKR, Responses, "<cr><lf>#VUR<cr><lf>",        1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>#VDT<cr><lf>",        1, 1b, 00, 00,00,00,00, 29,00,00,00

[VoiceV34]
HKR, LineSetRecordFormat,     1,, "at#vsm=2<cr>"
HKR, LineSetRecordFormat,     2,, "at#vsc=0<cr>"
HKR, LineSetRecordFormat,     3,, "at#vss=2<cr>"
HKR, LineSetRecordFormat,     4,, "at#vl=0<cr>"
HKR, LineSetRecordFormat,     5,, "at#vg=191<cr>"
HKR, LineSetRecordFormat,     6,, "at#vab=2<cr>"
HKR, LineSetRecordFormat,     7,, "at#vbo=1<cr>"
HKR, LineSetRecordFormat,     8,, "at#vti=0<cr>"
HKR, LineSetRecordFormat,     9,, "at#vsi=120<cr>"

HKR, HandsetSetRecordFormat,  1,, "at#vsm=2<cr>"
HKR, HandsetSetRecordFormat,  2,, "at#vsc=0<cr>"
HKR, HandsetSetRecordFormat,  3,, "at#vss=2<cr>"
HKR, HandsetSetRecordFormat,  4,, "at#vl=0<cr>"
HKR, HandsetSetRecordFormat,  5,, "at#vg=191<cr>"
HKR, HandsetSetRecordFormat,  6,, "at#vab=2<cr>"
HKR, HandsetSetRecordFormat,  7,, "at#vbo=1<cr>"
HKR, Sierra\TrainingQuery,  Response     ,, "<cr><lf>#SPT=2<cr><lf><cr><lf>OK<cr><lf>"

[Strings]
Sierra = "Sierra Semiconductor"
Modem1="Sierra 14.4 Data Fax SQ3223"
Modem2="Sierra 14.4 Data Fax Voice SQ3229"
Modem3="Sierra 14.4 Data Fax Voice SQ3262"
Modem4="Sierra 14.4 Data Fax Voice SQ3228"
Modem5="14.4 Data Fax"
Modem6="Sierra 14.4 Data Fax Voice SQ3230"
SQ3465 = "Sierra 28800 PnP SQ3465"

[All]
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init, 1,, "AT<cr>"
HKR, Responses, "<cr><lf>OK<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00

[INTERNAL]
HKR,, DeviceType, 1, 02

[MfgAddReg]
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Init, 2,, "AT &F E0 V1 &C1 &D2 W2 \V1<cr>"
HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Hangup, 1,, "ATH<cr>"
HKR, Answer, 1,, "ATA<cr>"
HKR,, Reset,, "ATZ<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ";"
HKR, Settings, SpeakerVolume_Low,, "L0"
HKR, Settings, SpeakerVolume_Med,, "L2"
HKR, Settings, SpeakerVolume_High,, "L3"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, FlowControl_Off,, "&K0"
HKR, Settings, FlowControl_Hard,, "&K3"
HKR, Settings, FlowControl_Soft,, "&K4"
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N4"    
HKR, Settings, ErrorControl_On,, "\N3"
HKR, Settings, Compression_Off,, "%%C0"
HKR, Settings, Compression_On,, "%%C1"
HKR, Settings, Modulation_CCITT,, "B0 " 
HKR, Settings, Modulation_Bell,, "B1"
HKR, Settings, SpeedNegotiation_Off,, "N0"
HKR, Settings, SpeedNegotiation_On,, "N1"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, Blind_Off,, "X4"
HKR, Settings, Blind_On,, "X3"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, InactivityTimeout,, "\T<#>"
HKR,Responses,"+FCERROR",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"+FCON",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr>",1,01,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>BUSY<cr><lf>",1,06,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT<cr><lf>",1,02,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>ERROR<cr><lf>",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO ANSWER<cr><lf>",1,07,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO CARRIER<cr><lf>",1,04,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO DIALTONE<cr><lf>",1,05,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>OK<cr><lf>",1,00,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>RING<cr><lf>",1,08,00,00,00,00,00,00,00,00,00
HKR,Responses,"<lf>",1,01,00,00,00,00,00,00,00,00,00
HKR,Responses,"0<cr>",1,00,00,00,00,00,00,00,00,00,00;OK
HKR,Responses,"2<cr>",1,08,00,00,00,00,00,00,00,00,00;RING
HKR,Responses,"3<cr>",1,04,00,00,00,00,00,00,00,00,00;NOCARRIER
HKR,Responses,"4<cr>",1,03,00,00,00,00,00,00,00,00,00;ERROR
HKR,Responses,"6<cr>",1,05,00,00,00,00,00,00,00,00,00;NODIALTONE
HKR,Responses,"7<cr>",1,06,00,00,00,00,00,00,00,00,00;BUSY
HKR,Responses,"8<cr>",1,07,00,00,00,00,00,00,00,00,00;NOANSWER
HKR,Responses,"BLACKLISTED",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"BUSY",1,06,00,00,00,00,00,00,00,00,00
HKR,Responses,"CARRIER 1200",1,01,00,B0,04,00,00,00,00,00,00
HKR,Responses,"CARRIER 1200/75",1,01,00,B0,04,00,00,00,00,00,00
HKR,Responses,"CARRIER 12000",1,01,00,E0,2E,00,00,00,00,00,00
HKR,Responses,"CARRIER 14400",1,01,00,40,38,00,00,00,00,00,00
HKR,Responses,"CARRIER 2400",1,01,00,60,09,00,00,00,00,00,00
HKR,Responses,"CARRIER 300",1,01,00,2C,01,00,00,00,00,00,00
HKR,Responses,"CARRIER 4800",1,01,00,C0,12,00,00,00,00,00,00
HKR,Responses,"CARRIER 7200",1,01,00,20,1C,00,00,00,00,00,00
HKR,Responses,"CARRIER 75/1200",1,01,00,B0,04,00,00,00,00,00,00
HKR,Responses,"CARRIER 9600",1,01,00,80,25,00,00,00,00,00,00
HKR,Responses,"COMPRESSION: CLASS5",1,01,03,00,00,00,00,00,00,00,00
HKR,Responses,"COMPRESSION: MNP5",1,01,03,00,00,00,00,00,00,00,00
HKR,Responses,"COMPRESSION: NONE",1,01,00,00,00,00,00,00,00,00,00
HKR,Responses,"COMPRESSION: V.42BIS",1,01,03,00,00,00,00,00,00,00,00
HKR,Responses,"CONNECT",1,02,00,00,00,00,00,00,00,00,00
HKR,Responses,"CONNECT/REL",1,02,02,00,00,00,00,00,00,00,00
HKR,Responses,"CONNECT 0300/REL",1,02,02,2C,01,00,00,00,00,00,00
HKR,Responses,"CONNECT 115,200",1,02,00,00,C2,01,00,00,00,00,00
HKR,Responses,"CONNECT 115,200/REL",1,02,02,00,C2,01,00,00,00,00,00
HKR,Responses,"CONNECT 115200",1,02,00,00,C2,01,00,00,00,00,00
HKR,Responses,"CONNECT 115200/REL",1,02,02,00,C2,01,00,00,00,00,00
HKR,Responses,"CONNECT 1200",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"CONNECT 1200/75",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"CONNECT 1200/REL",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"CONNECT 12000",1,02,00,E0,2E,00,00,00,00,00,00
HKR,Responses,"CONNECT 12000/REL",1,02,02,E0,2E,00,00,00,00,00,00
HKR,Responses,"CONNECT 14400",1,02,00,40,38,00,00,00,00,00,00
HKR,Responses,"CONNECT 14400/REL",1,02,02,40,38,00,00,00,00,00,00
HKR,Responses,"CONNECT 16800",1,02,00,A0,41,00,00,00,00,00,00
HKR,Responses,"CONNECT 16800/REL",1,02,02,A0,41,00,00,00,00,00,00
HKR,Responses,"CONNECT 19200",1,02,00,00,4B,00,00,00,00,00,00
HKR,Responses,"CONNECT 19200/REL",1,02,02,00,4B,00,00,00,00,00,00
HKR,Responses,"CONNECT 21600",1,02,00,60,54,00,00,00,00,00,00
HKR,Responses,"CONNECT 21600/REL",1,02,02,60,54,00,00,00,00,00,00
HKR,Responses,"CONNECT 2400",1,02,00,60,09,00,00,00,00,00,00
HKR,Responses,"CONNECT 2400/REL",1,02,02,60,09,00,00,00,00,00,00
HKR,Responses,"CONNECT 24000/REL",1,02,02,C0,5D,00,00,00,00,00,00
HKR,Responses,"CONNECT 26400",1,02,00,20,67,00,00,00,00,00,00
HKR,Responses,"CONNECT 26400/REL",1,02,02,20,67,00,00,00,00,00,00
HKR,Responses,"CONNECT 28800",1,02,00,80,70,00,00,00,00,00,00
HKR,Responses,"CONNECT 28800/REL",1,02,02,80,70,00,00,00,00,00,00
HKR,Responses,"CONNECT 300REL",1,02,02,2C,01,00,00,00,00,00,00
HKR,Responses,"CONNECT 38400",1,02,00,00,96,00,00,00,00,00,00
HKR,Responses,"CONNECT 38400/REL",1,02,02,00,96,00,00,00,00,00,00
HKR,Responses,"CONNECT 4800",1,02,00,C0,12,00,00,00,00,00,00
HKR,Responses,"CONNECT 4800/REL",1,02,02,C0,12,00,00,00,00,00,00
HKR,Responses,"CONNECT 57600",1,02,00,00,E1,00,00,00,00,00,00
HKR,Responses,"CONNECT 57600/REL",1,02,02,00,E1,00,00,00,00,00,00
HKR,Responses,"CONNECT 7200",1,02,00,20,1C,00,00,00,00,00,00
HKR,Responses,"CONNECT 7200/REL",1,02,02,20,1C,00,00,00,00,00,00
HKR,Responses,"CONNECT 75/1200",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"CONNECT 9600",1,02,00,80,25,00,00,00,00,00,00
HKR,Responses,"CONNECT 9600/REL",1,02,02,80,25,00,00,00,00,00,00
HKR,Responses,"DATA",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"DELAYED",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"DIALING",1,01,00,00,00,00,00,00,00,00,00
HKR,Responses,"ERROR",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"FAX",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"NO ANSWER",1,07,00,00,00,00,00,00,00,00,00
HKR,Responses,"NOANSWER",1,07,00,00,00,00,00,00,00,00,00
HKR,Responses,"NO CARRIER",1,04,00,00,00,00,00,00,00,00,00
HKR,Responses,"NOCARRIER",1,04,00,00,00,00,00,00,00,00,00
HKR,Responses,"NO DIALTONE",1,05,00,00,00,00,00,00,00,00,00
HKR,Responses,"NODIALTONE",1,05,00,00,00,00,00,00,00,00,00
HKR,Responses,"OK",1,00,00,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: ALT",1,01,02,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: ALTERNATE,",1,01,02,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: ALTERNATE,<cr><lf>CLASS2",1,01,02,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: ALTERNATE,<cr><lf>CLASS2+CLASS4",1,01,02,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: ALTERNATE,<cr><lf>CLASS2+CLASS4+CLASS5",1,01,03,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: ALTERNATE,<cr><lf>CLASS3",1,01,02,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: ALTERNATE,<cr><lf>CLASS3+CLASS4",1,01,02,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: ALTERNATE,<cr><lf>CLASS3+CLASS4+CLASS5",1,01,03,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: LAP-M",1,01,02,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: NONE",1,01,00,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: V.42",1,01,02,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: V.42BIS",1,01,03,00,00,00,00,00,00,00,00
HKR,Responses,"PROTOCOL: V42BIS",1,01,03,00,00,00,00,00,00,00,00
HKR,Responses,"RING",1,08,00,00,00,00,00,00,00,00,00
HKR,Responses,"RINGING",1,01,00,00,00,00,00,00,00,00,00
HKR,Responses,"UN-OBTAINABLENUMBER",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"VOICE",1,03,00,00,00,00,00,00,00,00,00

[PreCopySection]
HKR,,NoSetupUI,,1

[DLL_FILES]
spktrn32.dll
spktrn16.dll

[DestinationDirs]
Register.Copy    = 17     ;LDID_INF
DLL_FILES        = 11    
